PACKING LIST:  ELEVATOR

•	MOTOR PLATE TO LIFT:
       (4) 1.5 x ½” HEX BOLTS (4) ½” WASHERS (4) ½” LOCK NUTS
•	MOTOR SPACERS:
       (2) 2” PIPE 5 ½” LONG WITH A ½” HOLE
•	BUNK BRACKETS & HARDWARE:
       (8) 2” X 2” ANGLE WITH 2 HOLES ON ONE SIDE AND 2 HOLES ON THE OTHER SIDE   
       OF THE ANGLE.  (24) 3/8: HEX BOLTS (16) 3/8: WASHERS (8) LOC WASHERS (24) NUTS
•	GUIDE POST:
       (2) 10” X 12” FLAT PLATE WITH WELDED 2” BEARING TO HOLD WEIGHT PIPE AND 
       P.V.C.  IT HAS (4) 3/8: HOLES.  (8) 3/8” LOC WASHER (4) ANGLED
•	PULLEYS AND AXLE BOLTS:
       (2) BOLTS (2) LOC NUTS (2) PULLEYS
•	BUNKS:
       EITHER (2) CARPETED BOARDS OR (2) ALUMINUM BUNKS
•	CRADLE ARMS THAT HOLD BOAT (2) (L) SHAPED:
•	TRACKS:
       (2) I BEAMS FROM 20’ LONG TO 30’ LONG DEPENDING ON ORDER.
•	CABLES:
       (2) CABLES
•	CROSS BRACING AND HARDWARE:
       10 K (2) 12’ LONG 3” X 3” X 3/8” ANGLE
       13K & 16K (6) PIECES 3” X 3” X 3/8” ANGLE
       EACH PIECE TAKES (2) 1.5” X 3/8” HEX BOLT (2) 3/8: NUT
       (2) 3/8: LOC NUT
•	TOP CARRIERS:
       (2) COMPLETE WITH CABLE WINDERS
       (8) ½” X 1 ¾ “ HEX BOLTS (8) ½” LOC NUTS
•	DEADMAN:
       (2) ANGLED PIECES FROM 5” TO 7” DEPENDING ON THE SIZE OF THE LIFT.  (6) 3/8” X   
       1.5” HEX BOLTS (6) LOC NUTS
•	CABLE CLAMPS:
       (2) CABLE CLAMPS TO HOLD CABLE IN PIPE
•	COVERS:
       (2) COVERS (4) 1.5” HEX BOLTS (4) WASHERS (4) NUTS (2) SQUARE PLATES WITH   
       OBLONG HOLES (4) WASHERS WITH WELDED PINS
•	DRIVE UNITS:
       (2) DRIVE PLATES (2) 10” PULLEYS (2) 2” PULLEYS (2) BELTS (2) SWITCHES WITH 
       G.F.I.  OR (1) REMOTE (OPTIONAL)
•	GUIDE POST AND PIPES:
       (2) P.V.C PIPES WITH CAPS (2) 4’ WEIGHT PIPES 1.5” ROUND
•	DEADMAN BOLTS FOR 13K THRU 16KLB LIFTS:
       (2) 2.5” X ½” BOLTS (2) ½” WASHERS (2) LOC NUTS
       IF CIRCLED YOU HAVE ORDERED THE OPTIONAL PRODUCT AND IT SHOULD BE   
       INCLUDED WITH YOUR ORDER:
•	KICKER BRACE:
       FOR SPANS OF OVER 13; YOU NEED (2)
•	ZINCS:
       (1) MUSHROOM STYLE WITH (1) ½” X 1” HEX BOLT (1) ½” LOC WASHER

•	WALK BOARD			QTY: (   )
•	MOUNTING HARDWARE		QTY: (   )
•	STERN PLATFORM			QTY: (   )
•	WHEELS ALUMINUM		QTY: (   )
•	WHEELS NYLON			QTY: (   )
•	EXTRA ZINCS			QTY: (   )
•	SIDE MOUNT BRACKETS		QTY: (   )
EACH BRACKET SHOULD INCLUDE (2) 1/5 X 3/8 BOLTS WITH NUTS AND LOC WASHERS